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Thank you for your interest in Wulftec quality stretch wrapping solutions. Over the years, Wulftec’s rugged machine design has set the standard for the stretch wrap industry.

We propose the SML-200 model, a standard base low-profile turntable as the ideal stretch wrapping solution for your unique needs. Expect to improve productivity, operator efficiency while reducing film and labor costs.   
Our quotation includes the following information: 
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3
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Section 1 - The Wulftec Advantage
Wulftec Stretch Wrappers Give You the Most Value for Your Money

As a distributor or end-user, it’s important to compare what’s available before choosing your equipment provider.

It’s also important to get the best value for your investment. Why save a few bucks on a stretch wrapper if it can’t handle the workload? A stretch wrapper that constantly breaks down can’t guarantee a secure wrap, and it certainly won’t help you ship products on time. 

When it comes to strength and flawless performance, no other manufacturer can compare to Wulftec. That’s because only Wulftec stretch wrappers are backed by the Wulftec Advantage. Just ask any end-user who relies on a Wulftec stretch wrapper to keep end-of-line production rates at maximum efficiency: You simply can’t get better value for your money.
Unique To Wulftec
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All-steel structures
Wulftec is the only manufacturer of stretch wrap equipment that attaches a significant importance to strength. We don’t want you calling in five years to tell us that the structure has been compromised—for whatever reason. All Wulftec structures are built with heavy-duty steel for rugged performance, in even the harshest work environments. They’re built strong to last forever.
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AC variable frequency drives
Wulftec was the first in North America to put AC variable frequency drives as standard equipment on all machines. Why? Lower maintenance and better reliability—Wulftec stretch wrappers will save you time and money.
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Pre-Stretch Profitability

Wulftec’s NO-THREAD® Powered Pre-Stretch carriage allows film to be stretched up to 300% for optimal film use and reduced costs—without compromising wrap strength and consistency. Our carriage is a true NO-THREAD for enhanced safety.
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Warranties

Wulftec is the only manufacturer to offer a LIFETIME warranty on its pre-stretch rollers’ blue compound. Plus, all Wulftec stretch wrap machines feature a 5-year unlimited cycle warranty and 10-years on the steel structure.
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Non-proprietary parts

Wulftec is one of the few manufacturers to offer the convenience of non-proprietary parts throughout, which means they are easily accessible on a local basis.
Technical Support

The industry’s best-built products…
…backed by superior customer service

We won’t settle for anything less than 100% customer service. No matter what your needs are or where you are located.

Behind every Wulftec product, you benefit from:
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Experienced sales representatives and local distributors

· A highly-trained customer service team
· Technicians who offer on-site service and additional internal support

· A dedicated individual to handle customer requests and technician scheduling

· An entire organization that puts customer service front and center!
To serve you better, Wulftec has:

· A Wulftec school where distributors are trained on each piece of machinery. Training includes: servicing, installation and start-up, programming.
· Inventory throughout the world to support after-sales service

· Strategic parts depot programs in the United States and Canada

· A strong network of qualified distributor partners positioned close to our customers

· Attentive customer service

· Toll-free 1-877-WULFTEC (1-877-985-3832) or (819) 838-4232
· After hours technical assistance for emergencies
Technical Expertise
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Dedicated employees recruited from high-tech schools and universities

· Solution-oriented engineers who are ready to tackle any packaging challenge.

· Engineering team constantly creating new designs and improvements to meet customer needs

· Investment of time and money for ongoing research.
· Working closely with top brands such as Rockwell, SMC, Sick, and Baldor, to always get the best of their products and be the first to integrate new technologies.
· A team with one mindset: be ahead of the game!
Section 2 - Features & Benefits

Over the last several years, Wulftec's rugged machine design has set the standard for the stretch wrap industry.  We are confident that this offer will meet your requirements as far as performance, durability, safety, and affordability are concerned.
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LEASE WULFTEC® PACKAGING EQUIPMENT
WITH NO MONEY DOWN!

Why Wait For A Better Bottom Line To Invest In Quality Packaging Equipment? Instead, Lease
Walftec Packaging Equipment And Get More For Less.

Benefittoday from 100% financing and a $1 end-of-ease purchase option!

‘Wuiftecs leasing program i ight for you i

« Youare 2 Wulftec distrbutor or an end-user
» You need up to 100% financing.

» You want high-quality equipment but currently dor't have the funds

» You wouldlike the option of keeping the equipment a the end of your lease

Leasing It Makes Sense!

» Wite oflease payments as an operating cost
« Enjoy flexible payments.

= Preserve cash flow for other business needs

= Afford equipment that's fater, more effcient and more accurate, but expensive to buy outright
= Spread out the cost of equipment over several years

= Keep your creditlines and borrowing potentialintact

* Improve your equiy-to-deb ratio

Save Even More Time And Money With Our $1 Purchase Option!

At the end of your lease, purchase your Walftec packaging equipment for only $11 That's ight, you get to keep the
machine..and enjoy relable, efficint packaging equipment for years to come (after al it’s a Wulftec 50 its made o last).

= No need to spend man hours shopping around for new equipment
» No downtime related to replacing the machine with another one
* Increase workforce efficiency

Attention Wulftec Distributors — This Offer is For You!
Benefit rom our easing program to filyour showroom with Wftec packaging equipmen.
Clients who see Wulftec packaging equipment buy Wulftec packaging equipmen.

For more information,

« Visit our website at s wuifec com

= Email us at: wuiftec @wlftec com

» Call olifree: 1877 WULFTEC (985-3832)

WWW.WULFTEC.COM
WE FEAR NO PACKAGING CHALLENGE

= DURAVANT




The proposed model incorporates many standard features including:

· 5,000 lbs. load weight capacity 
· NEMA 4/12 control panel dust tight and waterproof
· Our control panel is UL508A approved from factory
· 100% Heavy duty structural steel construction 
· Superior Electrical/Control design including Allen Bradley PLC
· Wulftec’s exclusive 20” NO-THREAD® Powered Pre-Stretch Carriage (30” optional)
· Lifetime warranty on pre-stretch rollers blue compound
· Readily available non-proprietary parts
· State-of-the-art electrical control panel with all finger safe electrical components
· Carriage lifting chains enclosed inside tower for operator safety
Some of the standard features are listed below: 

Carriage

NO-THREAD® Powered Pre-Stretch film delivery system. Designed with safety in mind, no film threading is required and a Lexan cover prevents access to the rollers when gate is closed. Our linear device compensates for corners to provide even film tension on the load.  The “Maintenance Free” spring loaded carriage gate equipped with spring loaded rollers, ensures optimal contact with the stretch film year after year, without involving maintenance. Preset pre-stretch ratios are available ranging from 50-300%, std. is 200%.
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Allen Bradley AC Variable Frequency Drives
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The SML-200 is equipped with Allen Bradley Powerflex 525 series drives for lower maintenance and better reliability. 
1. AC motors do not require periodic inspection and replacement of brushes as required on DC motors.

2. Allow soft start/stop for smooth operation.

3. AC drives include a digital read-out, which allows monitoring of speed, current and voltage. Thus, fine tuning is made easier and more reliable compared to DC drive trim pots.

4. AC drives include internal diagnosis, fault alarms and power surge protection.

5. AC drive’s power components are enclosed inside a drive case, thus providing service personnel safer access inside the control panel.  
NEMA 12 Control Cabinet
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Deluxe panel shown above
	Operating Controls

· Allen Bradley Micro 800 series PLC

· Sick autoheight Photoeyes

· 24V Control System

· Power on/off switch
and indicator light

· Current overload protection

· Reset function
· Emergency stop button

· 230VAC/3PH/60HZ Motors
and 120VAC/1PH/60HZ                     Allen Bradley Power Flex 525
Variable Frequency Drives


Section 3 - Standard Specifications                     
	Production Rate
	Up to 55 loads per hour based on load configuration and machine options.

	Machine Dimensions
	119 ½” L x 66” W x 86 3/8” H – based on 80” wrap height

	Load Size
	55"L x 55"W x 80”H (78” diagonal) - other wrap heights available

	Load Weight
	5,000 lbs. 

	Approx. Shipping Weight
	2,500 lbs.

	Electrical Requirements
	120V/1/60 15A

	Controls
(Refer to “description of Control Panel” page)
	Allen Bradley Micro 800 series PLC
24V control system
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Current overload protection 

NEMA 4/12 control cabinet 
UL 508A certified control panel from factory
Sick autoheight sensing photoeye with on/off mode

Power indicator light (Basic)*
Power on/off switch and status light (Standard)*
Start/stop push button
Large Emergency Stop (push pull type)
Manual carriage up/down function
Variable rotation speed (16 RPM) with automatic home position
Carriage speed adjustment
Top and bottom wrap selections 
Reinforced wrap/manual rotation control
Film force to load control

Lack of film alarm

	Structure
	14 gauge formed steel tower

Forklift portable base design (from back only)

Heavy duty structural steel construction
10 year warranty on steel structure

	Film Delivery System
	20" NO-THREAD® Powered Pre-Stretch (no film threading)

1 HP Motor & PowerFlex AC variable frequency drive
Lifetime warranty on pre-stretch rollers blue compound

Film force release for easy pull at start and end of cycle

50-300% pre-stretch ratio (preset to customer specs – std. 200%)
Electronic film tension control with analog sensor

Tower mounted film roping bar
Lexan roller cover for operator safety
Proximity sensor on carriage gate to ensure gate is properly closed

	Film Carriage Drive


	1 HP AC motor with Allen Bradley PowerFlex variable frequency drive

Two #50 carriage lifting chains

Bearing supported maintenance   free guide wheels


	Turntable
	65” dia. 3/8” steel plate

32 heavy duty non-metallic lube-free table supports

3” table height

2 3/8” high base

Ramp accessible on all three sides (consult factory when ordering more than one ramp)

	Turntable Drive
	0-16 RPM variable speed

1 HP AC motor with Allen Bradley variable frequency drive

#50 ANSI heavy duty chain drive

Electronic soft start/stop

Positive turntable alignment controlled by proximity sensor

	Technical Information
	The machine is provided with a manual including electro/mechanical schematics and drawings, troubleshooting guide & installation instructions


If pit mounting – please consult factory

* see Section 8 for complete panel descriptions

For machines shipping outside continental USA and Canada, consult factory

Section 4 – Load Sizes and Production rates
We have designed your system according to the following specifications:
Wulftec Maximum Load Sizes

	
	Diagonal
	Length
	Width
	Height
	Weight

	Maximum
	78”
	55”
	55”
	80”
	5,000 Lbs.


Customer Load Sizes

	
	Diagonal
	Length
	Width
	Height
	Weight

	Maximum
	
	
	
	
	

	Minimum
	
	
	
	
	


Production Rate
	Loads per hour wrapping at 16 RPM

	Loads Per Hour
	Total Rotations
	Top Wraps
	Bottom Wraps
	Overlap Up/Dn
	Overwrap
	Carriage Size
	Load Height

	42 lph
	11
	2
	2
	2" & 2"
	2"
	20"
	60"

	49 lph
	8
	2
	2
	2" & 2"
	2"
	30"
	60"


	Loads per hour wrapping at 16 RPM

	Loads Per Hour
	Total Rotations
	Top Wraps
	Bottom Wraps
	Overlap Up/Dn
	Overwrap
	Carriage Size
	Load Height

	39 lph
	13
	2
	2
	2" & 2"
	0"
	20"
	80"

	47 lph
	9
	2
	2
	2" & 2"
	0"
	30"
	80"


* includes 30 seconds for operator intervention 
Section 5 - Your System’s Description & Prices

Pricing

	SML-200 Semi-Automatic Low Profile – Smart Series
	$14,865.00

	1. 
	65” diameter turntable with full surround (5000 lbs. capacity)
	Included

	2. 
	80” Wrap height 
	Included

	3. 
	20” NO-THREAD® powered pre-stretch carriage - 200% pre-stretch ratio with Maintenance Free spring loaded carriage gate 
	Included

	4. 
	Variable rotation speed up to 16 RPM with automatic home position


	Included

	5. 
	Allen Bradley PowerFlex 525 AC frequency Drives and Baldor Motors.
	Included

	6. 
	Basic control panel including:
	· Allen Bradley Micro 800 series PLC

· Basic wrapping functions including:

· Top and bottom wrap selectors (1-3)

· Turntable speed adjustment

· Carriage speed adjustment

· Film tension adjustment

· Manual mode carriage up/down

· Autoheight sensing photoeye on/off

· Reinforce wrap/manual rotation
	Included

	7. 
	1 x Operational manual (including installation instructions) 
	Included


If film gauge is above 1 mil, please indicate it on purchase order as modifications to the prestretch mechanism are required.  Additional charges may apply.  
	BUDGET QUOTATION
	
	SalesName

	Survey questionnaire required
	
	SalesTitle


	Customization package 

	8. 
	200% pre-stretch ratio, belt and pulley driven, is Wulftec’s standard for semi-automatic machines. If a different pre-stretch is required, it must be indicated in PO.
	N/C

	9. 
	
	

	10. 
	
	

	11. 
	
	

	12. 
	
	

	13. 
	
	

	14. 
	
	

	15. 
	
	

	16. 
	
	

	17. 
	
	

	18. 
	
	

	19. 
	
	

	20. 
	
	

	21. 
	
	

	22. 
	
	

	23. 
	
	

	24. 
	
	

	25. 
	
	


	Total Pricing: 

	Customization Pkg. Price: 
	

	Basic System Price: 
	$14,865.00

	Total System Price: 
	


Note:  The above proposal does not include the Performance Level d (PLd) Safety package.
Refer to Section 6 for full details on the safety package.
	BUDGET QUOTATION
	
	SalesName

	Survey questionnaire required
	
	SalesTitle


Section 6 – Safety Requirements
NOTE: This section must be present in all proposals when presented to the end users.

Performance Level d (PLd) Safety Package*

Includes Category 3 safety circuitry and components that meet or exceed the requirements for PLd.

Your safety package consists of:

	Safety Multibeam Sensor

	SICK deTem4 safety multibeam sensors to protect the entrance of the process area from human intrusion.  The control enclosure is mounted on a stand to be located outside of the fencing.
Includes the addition of a safety relay to monitor and control the safety circuit and a redundant contact E-stop circuit.

 A 2-button lanyard with E-stop button is provided to rearm the safety circuit and start the machine operation.
After the forklift driver places the load in the wrap zone, he must back out of the wrap zone clearing the safety multibeam sensors, verify that the wrap zone is clear of all personnel, and then re-arm the safety circuit on the lanyard and start the cycle.

If the safety multibeam sensor barrier is broken at any time during the cycle the machine will stop and will not be able to restart until the safety relay has been reset.

The pre-stretch motor will not be powered when in an E-stop condition or when the wrap zone entrance has been breached. Film can still be easily pulled out of the carriage by opening the carriage gate.  Options are available to disengage the pre-stretch rollers to allow the film to be pulled through without opening the gate; see Section 7.
	$9,435.00


	Safety Fencing

	3-sided safety fencing around process area.  Fencing is heavy duty with Safety Yellow support posts and Black wire mesh sections for improved visibility into the wrap zone.  The overall height of the fencing is 87” from the floor, with a 5.5” sweep space under the panels.  This fencing kit is installed with a distance of 39” between the multibeam sensor and the nearest hazardous movement and does not meet the requirements for safe distances based on ISO13855, CSA Z432-16, and ANSI B11.19.  Refer to the Safety Fence Extensions below and the notes on the following page
	$6,645.00


	Safety Fence Extensions

	Extensions to the standard safety fencing kit and multibeam sensor cabling to meet the requirements for safe distances in ISO13855, CSA Z432-16, and ANSI B11.19.  This positions the multibeam sensor 225” from the nearest hazardous movement.
	$3,360.00

	TOTAL SAFETY PACKAGE COST
	$19,440.00


	Electric dump valve

(required when adding an option with pneumatic components)  

	SMC CAT 3 electric dump valve to purge the pneumatic system (including the cylinders) when an E-stop is pressed or process area entrance is breached (fence key switch and/or safety multibeam sensors), as well as when the machine power is disconnected. 
Note: Air supply to clamp will not be available during e-stop situations; the clamps spring loaded design allows the clamp to hold the film in place, yet it is easy to manually open and close for film loading.
	$2,470.00


Important Notes:

1. This safety package has been designed to respond to the requirements of ISO13855, CSA Z432-16, and ANSI B11.19.  The contents of the safety package are based on the equipment and features included in the customization package above.    Any additional options or modifications to the layout may affect safety package pricing.  

2. If any portion of this safety package is not purchased with the equipment, or if the customer chooses to supply and integrate their own safety package rather than purchasing from Wulftec, they engage to provide the equivalent or greater than what is quoted here, they understand that these important safety aspects will then be their responsibility, and they relieve Wulftec from all responsibility.

3. In certain instances the integration of the safety package may affect the cycle time.
Section 7 - Options

	Height Extension Options

	1. 
	Increase wrap height to 92”
	$1,010.00

	2. 
	Increase wrap height to 104”
	$1,220.00

	3. 
	Increase wrap height to 116”
	$1,430.00

	4. 
	Increase wrap height to 128”
	$1,840.00


	Control Panel Options

	5. 
	Upgrade from BASIC to STANDARD control panel
	$430.00

	6. 
	Upgrade from BASIC to STANDARD PLUS control panel
	$1,270.00

	7. 
	Upgrade from BASIC to DELUXE control panel
	$3,650.00

	see Section 8 for complete description


	Carriage Options

	8. 
	Upgrade to 30” NO-THREAD powered pre-stretch carriage.  Includes the conversion of Baldor motor to JIE brake motor on carriage up/dwn
	$1,460.00

	9. 
	Tilting carriage mandrel to allow the operator to tilt the film roll mandrel to a convenient loading position.  Once loaded the mandrel folds back up and is locked into the operating position.  

Note:  Operator will need to manually raise the carriage to desired height before tilting mandrel.

Note:  may affect bottom wrap.  
	$2,335.00

	10. 
	Background suppression photoeye for dark or shiny loads autoheight detection.

Dual turntable requires 2
	$940.00/ea

	11. 
	Autoheight Adaptor Bracket

Autoheight adaptor bracket to run 20” film on a 30” carriage. This allows proper placement of the autoheight photoeye.
Dual turntable requires 2
	$480.00/ea

	12. 
	20” hydraulic carriage (No pre-stretch) to replace standard carriage (includes tension bypass)
	$770.00

	13. 
	30” hydraulic carriage (No pre-stretch) to replace standard carriage (includes tension bypass)
	$1,160.00


	Safety Package Film Feeding Options

	14. 
	Electric clutch to disengage the prestretch rollers between cycles allowing the operator to easily pull film from the carriage when the carriage is disabled by the safety circuit without having to open the carriage gate.  Can be used on carriages with prestretch ratios of 200% and higher.

Note: This option is only available when a safety controller or safety relay is purchased as part of the safety package.

Note: Not available with cold temperature B or C packages.
	$3,545.00

	15. 
	Enabling Switch for Prestretch.  Allows the operator to enable the prestrech carriage when the safety circuit is open, to be able to feed film at a low speed to attach the film to the load or to insert the film into the film clamp (if applicable).  The operator must hold the enabling switch to keep the prestretch engaged while they are pulling the film out.

Note: This option is only available when a safety controller or safety relay is purchased as part of the safety package.
	$2,855.00


	Film Tail Treatment Options

	16. 
	Rapid-cut feature for Basic panel

Save the operators one timely step in the wrapping process by adding a Rapid-Cut device to automatically puncture the film at the end of the cycle to separate the film from the load.

Note: Not available with hydraulic carriage, manual roping device, safety package or cold temperature B or C packages.

Note: Cannot be combined with a Smart Start Clamp.
	$1,665.00

	17. 
	Rapid-cut feature for Standard Panel

Save the operators one timely step in the wrapping process by adding a Rapid-Cut device to automatically puncture the film at the end of the cycle to separate the film from the load. 

Note: Not available with hydraulic carriage, manual roping device, safety package or cold temperature B or C packages.

Note: Cannot be combined with a Smart Start Clamp.
	$940.00

	18. 
	SMART™ Auto Start and Pull Cord

A manual clamping system holding the film in place at start of cycle, coupled with a pull cord to start the cycle without getting off of the forklift. This means the forklift driver only has to get off the forklift once per cycle.

Note: Cannot be combined with a Smart Start Clamp.
	$1,170.00


	Other Options

	19. 
	Smart 200 Loading Ramp
4’ x 6’, capacity 6,000 lbs.  This ramp has a 4’ gradual incline, a 2’ flat and is curved to fit turntable.
	$1,150.00

	20. 
	2ft ramp extension

The most common extension would be the two-foot flat.  This extension is fabricated in order that it may be attached to the existing standard ramp.

Note:  Certain walkies or pallet jacks require ramp extensions so please consult factory if your pallet jack/waklie is longer than standard or has long forks
	$775.00

	21. 
	Pull cord 

This pull cord allows the forklift driver to start and stop the machine.  It includes 60’ of cable and is activated by pulling once to start the cycle.  A second pull will interrupt the cycle.
	$915.00


	Miscellaneous Options

	22. 
	Each additional print copy of operating and instruction manual
	$160.00

	23. 
	Replace the standard printed manual with a downloadable digital copy.  A link to the manual will be sent at the time of shipment.
	N/C


All quoted prices are in US funds.
	Video FAT Options

	A Video FAT is an excellent way to reassure you that your equipment is complete and contains all of the features you require, avoiding unnecessary delays during the installation and startup of your new equipment.

Note that any Video FAT must be ordered on initial purchase order to allow for proper planning and scheduling with production.  FAT cannot be added once machine has been scheduled.  

To ensure customer product can be used during the Video FAT, refer to the Wulftec Video FAT Options document to understand test load shipment procedures, limitations, timing, and requirements. 

	1. 
	The Basic

A short, prerecorded video including a non-narrated walk-around of the equipment and control panel showing the components and any special options purchased.  Also includes a demo of the equipment in action.   

This video is for information only.  Machine will be packed once video and quality control have been completed.
	$415.00

	2. 
	The Standard

A fully narrated prerecorded video including a walk-around of the equipment and control panel showing the components and any special options purchased.  The narrator describes the features of the equipment and also includes a demo of the equipment in action.  

Due to the volume of orders in the production schedule, and limited floor space, the customer will have 24 hours to review and comment on the video.  If no reply is received within 24hrs, the video will be considered approved, and the machine will be shipped.
	$855.00


	3. 
	The Deluxe

The Deluxe Video FAT includes a fully narrated, prerecorded and downloadable video, customized based on specific requirements from the customer.  It may include specific checklists provided by you or a specific set of sequences that you wish to see that may not be included in the Standard or Basic Video FAT’s. 

The Deluxe Video FAT can also be conserved to be used as an operator training video to show new workers the basics of how to operate the system, how to navigate through the touch screen, and how to make simple adjustments. When requesting a quote for your Deluxe Video FAT, mention that you are interested in the operator training option.  Price typically ranges from $1,500 to $2,500 depending on what is requested in the video.

Due to the volume of orders in the production schedule, and limited floor space, the customer will have 24 hours to review and comment on the video.  If no reply is received within 24hrs, the video will be considered approved, and the machine will be shipped.
	TBD

	Note: If the Deluxe Video FAT purchased contains an instructional machine usage training portion, this portion of the video will be made available 1 to 2 weeks after the equipment has shipped and only the Standard portion will be made available for machine acceptance.  This allows the additional time necessary for video compilation without delaying machine shipment.


	BUDGET QUOTATION
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	SalesTitle


Section 8 – Description of Control Panels
	Basic Panel (included in machine price)
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	Features
	

	· Allen Bradley Micro 800 series PLC

· Allen Bradley PowerFlex 525 VFDs
	· Manual mode carriage up/down
	

	· Turntable rotation speed adjustable 0-16 RPM
	· Top & bottom wrap selector 1-3
	

	· Carriage up/down speed adjustment
	· Autoheight sensing photoeye on/off
	

	· Film tension adjustment
	· Start/Stop push button
	

	· Reinforced wrap
	· Power on light
	

	· Manual turntable rotation
	· Emergency Stop (push/pull)
	


	Standard Panel – allows for some options and minor program changes

	
	

	Features
	

	· Allen Bradley Micro 800 series PLC
· Allen Bradley PowerFlex 525 VFDs with safe off
	· Top cover on/off selector switch (splash-proof program)
· Reinforced wrap
	

	· Separate top and bottom wrap selectors 0-9
	· Autoheight sensing photoeye on/off
	

	· Film tension adjustment
	· Manual rotation
	

	· Rotation speed adjustable      0-16 RPM
	· Start/Stop push button
	

	· Separate up/down carriage speeds
	· Power On/Off switch and status light
	

	· Manual mode carriage up/down
	· Emergency stop (push/pull)
	

	· Spiral up/spiral up/down
	
	


	Standard PLUS Panel - Intuitive Touch Screen Interface
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	Features
	

	· All standard panel features as described above plus: 

· Allen Bradley Micro 800 series PLC
· Allen Bradley PowerFlex 525 VFDs with safe off
· PanelView 800 4.3” touch screen

· 3 pre-set wrap patterns

· Easy alarm readout

· Alarm log

· Step by step operation guidelines

· Password protection 

· 1 x light load and 1 x heavy load tension settings

· All speed and tension settings are adjustable in each wrap pattern
	


	Deluxe Panel – Allows for a full range of options and program changes

	
	

	Features
	

	· All standard panel features as described above plus: 

· Allen Bradley Micro 850

· Allen Bradley PowerFlex 525 VFDs with safe off
· Allen Bradley PanelView 800 7” 

· All pattern settings (speed and tension) are adjustable in each wrap pattern from HMI

· Loads per hour counter

· Non-resettable cycle counter

· 6 pre-set wrap programs

· Maintenance screen

· Alarm screen, troubleshooting guide and much more
	


Section 9 - Terms & Conditions
Transport

Ex Works Ayer's Cliff, Quebec, Canada for FOB Origin, freight prepaid and charged.

Unless prior and/or special arrangements have been made, the TRANSPORT EX WORKS AYER'S CLIFF, QUEBEC, CANADA ship point is Wulftec International’s plant, Ayer’s Cliff, Quebec, Canada. At this point, the title transfers and freight/insurance becomes the responsibility of the buyer. Ex Works means that the seller fulfills his obligation to deliver when he has made the goods available at his premises to the buyer. 

Shipping Date

Lead time will be communicated upon receipt of signed purchase order plus down payment (if required) and depending on production volume at that time.  Approval drawing requests will add approximately 2 weeks to the lead time.
Terms

100% Net 30 days after shipment.

20% cancellation fee applicable after 7 days.  No cancellation on orders that have shipped.
Purchase Orders over $40,000.00
40% non-refundable down payment together with signed purchase order
60% net 30 days after shipping. All applicable taxes will be added on this payment.
Purchase Order Acceptance Subject to Credit Approval. Payment terms may change at any time.

All applicable taxes will be added on the last payment.

All Merchandise Sold Hereby Will Remain the Property of Wulftec International Inc. until the Purchase Price Has Been Paid in Full.

Quote Valid for Thirty (30) Days.
We are confident you will find Wulftec International equipment to be not only rugged, reliable, safe and user friendly, but very affordable.  They are engineered to work right, and built to keep on working.

We appreciate this opportunity to address your needs and if you have any questions concerning this proposal, please call us.

Force Majeure: 
Neither Wulftec International nor Customer shall be liable for any delays or performance failures, other than Customer’s payment obligations, when such delays or failures are caused directly or indirectly by, without limitation, an act of God, war, mobilization, insurrection, rebellion, civil commotion, riot, act of an extremist or public enemy, sabotage, labor dispute, customs delay, lockout, strike, explosion, fire, flood, storm, accident, drought, power failure, inability to obtain suitable and sufficient energy, labor or material, delay of carriers, embargo, any existing or future law, ordinance, rule or regulation, whether valid or invalid, of the federal or of any state or foreign government affecting the conduct of business, including priority, requisition, allocation or price control; or due to any other cause beyond a party’s reasonable control, whether affecting procurement, production, transportation or any other phase related to an Order. Wulftec International shall also not be liable for any delays or performance failures caused directly or indirectly by the imposition of any new or increased tariffs, taxes, duties or similar charges by any governmental authority (whether federal, state or foreign), or by changes to economic conditions including but not limited to fluctuations in credit, debit, capital or financial markets, interest rates, exchange rates, or a significant increase in the cost of goods or services due to inflation (including as caused by new or increased tariffs) (as measured by the Consumer Price Index or a similar index), or any other changes in economic conditions and productivity (each, an “Economic Condition Change”).
Economic Condition Price Adjustment:

In the event of an Economic Condition Change, Wulftec International may, in its sole discretion, adjust the applicable pricing to reflect such changes. Wulftec International shall provide written notice to Customer of any such price adjustment.

	SalesName

	SalesTitle


Section 10 - Wulftec Smart Series Warranty

Wulftec International Inc. warrants its manufactured products for a period of five (5) years (with the exception of the components that are inside the Economy panel that are warranted for one (1) year). All 25” ring gear bearings that are warranted for ten (10) years to be free from manufacturing defects from the date of shipment if installed, maintained, and used in accordance with factory specifications. Wulftec International Inc. will, at its option, repair or replace any defective parts returned freight prepaid, subject to factory inspection and right to determine cause of failure. Damage caused by inadequate supply voltage, misuse, neglect or corrosive environment, is not covered by this warranty. The two (2) larger blue pre-stretch rollers carry a lifetime warranty on their blue compound. Damage in transport is the responsibility of the carrier and is not covered under our warranty.  All damages upon receipt of equipment should be reported immediately to the carrier and Wulftec International Inc. should be notified. This warranty only applies if machine start-up, modifications or repairs are made by an authorized Wulftec technician and does not cover workmanship at the customer’s site.
WULFTEC INTERNATIONAL INC. SHALL UNDER NO CIRCUMSTANCES BE LIABLE FOR ANY CONSEQUENTIAL DAMAGES, LOSSES OR EXPENSE ARISING IN CONNECTION WITH THE USE OF, OR INABILITY TO USE, OUR PRODUCT FOR ANY PURPOSE WHATSOEVER.  EXCEPT AS STATED HEREIN, WULFTEC INTERNATIONAL INC. MAKES NO OTHER WARRANTY, EXPRESSED OR IMPLIED, NEITHER DOES IT ASSUME NOR AUTHORIZE ANYONE ELSE TO ASSUME FOR IT, ANY OTHER OBLIGATION RELATING TO WULFTEC INTERNATIONAL INC. MACHINERY OR EQUIPMENT.  THIS WARRANTY DOES NOT APPLY TO EQUIPMENT WHICH, IN THE JUDGMENT OF WULFTEC INTERNATIONAL INC., HAS BEEN SUBJECT TO MISUSE, NEGLECT OR HAS BEEN STARTED-UP, REPAIRED OR ALTERED BY UNAUTHORIZED PERSONNEL.  DEFECTIVE PARTS MUST BE RETURNED TO WULFTEC INTERNATIONAL INC. WITHIN THIRTY DAYS (30) OF SHIPMENT OF A REPLACEMENT AND MUST BE RETURNED PREPAID IN THEIR ORIGINAL STATE.  FAILURE TO DO SO WILL VOID THE WARRANTY.  DEFECTIVE PARTS THAT HAVE BEEN DISASSEMBLED, DAMAGED DURING REMOVAL OR OTHERWISE TAMPERED WITH, WILL NOT BE COVERED UNDER WARRANTY, UNLESS OTHERWISE STATED IN WRITING BY WULFTEC INTERNATIONAL INC. WULFTEC INTERNATIONAL INC. MAKES NO WARRANTY AS TO FITNESS OF EQUIPMENT FOR PARTICULAR PURPOSES.  PRODUCTS SERVICED AND/OR PARTS REPLACED DURING WARRANTY PERIOD CARRY THE UNEXPIRED PORTION OF THE ORIGINAL WARRANTY ONLY.  WULFTEC INTERNATIONAL INC.'S SOLE OBLIGATION UNDER THIS WARRANTY WILL BE TO PROVIDE REPAIRS TO COMPONENTS OR REPLACEMENT PARTS; TRANSPORT EX WORKS AYER'S CLIFF, QUEBEC, CANADA.
Parts Returns
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IN CANADA
Wulftec International Inc.
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Disclaimer
Wulftec International Inc. has taken every precaution in the preparation of this document.  However, this information is subject to change without notice and is provided "as is" with no warranty.  Wulftec International shall not be liable for any direct, indirect, special, incidental or consequential damages in connection with the use of the information contained in this document.

Copyright
No part of this quote may be reproduced, in any form, in whole or in part without written permission of Wulftec International Inc.

Section 11 - Performance Guarantee

Equipment Capability

Your Wulftec stretch wrapper performance will meet production rates and load ranges specified in “Section 4 - Load Sizes and Production Rates” when properly maintained and supplied with quality materials and product, and operating with recommended parameter settings.  Wulftec is not responsible for the performance of the customer’s employees.

The Wulftec NO-THREAD® Powered Pre-Stretch carriage is capable of handling a variety of films from the lowest available gauge up to the highest.  Please advise Wulftec when using films from either extreme (below 60 gauge or above 1.2 mil) to be sure that any special features on the machine are properly adapted to wrap correctly with your film. 

The NO-THREAD® Powered Pre-Stretch is also capable of film pre-stretch from 50% to 300% (to be specified upon order).

Standards

Wulftec equipment is built per NEC, NFPA, and CEC, and the control panels are UL508A from factory (see our certification online at www.ul.com).  If any specifications and / or regulations related to a specific city or state are required, it will be the responsibility of the customer and / or the distributor to communicate the information to Wulftec so that the appropriate modifications and expenses can be added to the quotation.

Performance Guarantee

All Wulftec equipment will perform as stated in this document.

The quality of the “wrap” will be sufficient to prevent damage to the product under normal handling conditions and have dimensionally consistent overlaps.

If, for any reason, this equipment does not perform to these standards, we at Wulftec will make all necessary changes at no charge to the customer.

However, if it is found that the non-performance of the Wulftec equipment is due to the operational techniques of the customer’s operator(s) then the customer will be charged in full for the service call.

The performance test should take place immediately after installation and start-up.

Once the Performance Guarantee standards are satisfied, Wulftec’s responsibility under this Performance Guarantee will be deemed concluded.

The customer is responsible for the film quality and acknowledges that there is an optimal pre-stretch range required for best performance.

Notice of Adverse Events

The customer shall promptly notify Wulftec of any adverse event implicating bodily injury or property damages related to the use of Wulftec’s product.  Notice shall be given to the Customer Service Manager at wulftec@wulftec.com or at: (877) 985-3832.

Section 12 - Corporate Profile
Wulftec International Inc.:  A Tradition of Strength

Since 1990, Wulftec International Inc. has been synonymous for unbeatable strength and durability for stretch wrapping, strapping equipment and pallet handling solutions. We are renowned for developing, manufacturing and distributing the industry’s best-built equipment.  Our unwavering focus on quality, service and innovation means Wulftec® machines are designed to work flawlessly in any environment and under any condition, load after load, year after year.

Why are Wulftec® stretch wrappers, strapping equipment and pallet handling solutions considered to be the best? In addition to boasting unique patented features, every Wulftec comes with the Wulftec Advantage, which includes all-steel structural designs, AC variable frequency drives and the best warranties available. Behind every meticulously handcrafted Wulftec® machine are our highly skilled employees who work in our state-of-the-art facilities located just minutes from the Canadian-U.S. border and 75 miles from Montreal. We take pride in knowing that our commitment to excellence just can’t be beat.

Wulftec is a member of the DURAVANT family of companies. Duravant is a global engineered equipment company with manufacturing, sales and service facilities throughout North America, Europe and Asia. Through their portfolio of operating companies, Duravant delivers trusted end-to-end process solutions for customers and partners through engineering and integration expertise, project management and operational excellence. Being a member of the Duravant family strengthened Wulftec’s competitive advantage and ability to provide superior solutions to meet the individual needs of clients. Our strong entrepreneurial spirit dictates that if we haven’t built it yet, we’ll work with clients to build it now. This commitment to customer satisfaction goes well beyond equipment design. We also give equal attention to installation and operations training, after-sales service and maintenance.

Thanks to the can-do approach of Wulftec’s sales and service departments, along with our extensive network of Wulftec distributors, it’s easy for clients to benefit from the exceptional value, reliability and productivity that only Wulftec can offer.

For more information, contact us at 1-877-985-3832 or visit our website at www.wulftec.com. 
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